**ET1061 Failsafe**

This function dictates what the receiver will do if it loses signal from the

transmitter, this includes servo position etc.

**Setup:**

1. Turn on the transmitter and make sure it is connected to the receiver.

2. Hold the control surface at the desired failsafe position .

3. Press and hold the bind button for 3 seconds, if the G. LE D starts flashing every 2 seconds then setup has been successful.

Failsafe is now set and will default to the set values when the receiver loses signal .

Note: The fail-safe function has no default set at the factory and as such must be set manually.

If no failsafe setting has been set, then the receiver will not output anything when signal is lost.